ITP

**Description:**

This file contains all the information concerning the **Intergration** of global APIs with each other. Also containing the **timing Constrains** needed from the SRS.

**Version Information:**

Current Version: 1.1

Edited by : OMDA

Notes : In this version we added more details about each API integration with other layer APIs.

**Timing Test Cases:**

|  |  |  |  |
| --- | --- | --- | --- |
| REQ\_ITP\_001 | | | |
| Covers | TEST | EXPECTED | RESULT |
| REQ\_SRS\_017 | 1-Connect the Bluetooth Rx pin to Oscilliscope and send two consecutive signals | The time between receiving the first signal and the second signal should be 100 mSec with tolerance 5% |  |